{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":7,"n_cols":7,"rows_kept":7,"merged":[[0,0,0,6],[4,0,5,0],[6,0,6,1]]}
["郁南县人民医院医疗设备项目报价单"]
["序号","设备名称","技术参数","数量","单位","报价（单价）","总价（元）"]
[1,"超乳手柄+IA","1、可反复多次消毒使用。\n2、纵向超声模式。\n3、可搭配 19G、20G、21G 超乳针头。\n4、可匹配WHITESTAR白星超乳技术\n5、适配我院 眼力健 COMPACT 超声乳化仪。",2,"套"]
[2,"人体成人分析仪","1.测量原理和方法：8点接触式电极，多回路方法，生物电阻抗法\n2.测量指标：应包含全身脂肪含量、全身肌肉含量、躯干脂肪含量、躯干肌肉含量和骨质含量\n3.可进行内脏脂肪面积指标分析\n4.有语音指示下，自动进行体重和人体成分的测量，测量完成后自动生成人体成分报表\n5.阻抗测量范围：150Ω~1200Ω，阻抗测量精度：≦±12Ω\n6.可升级同品牌超声多普勒血流检测仪\n7.可升级同品牌肌电图仪进行神经传导数据采集、处理和分析\n8.使用期限≧10年",1,"台"]
[3,"可视喉镜","1.摄像头与喉镜片前端的距离适中，无盲区，气管插管操作更精准。 \n2.高清晰真彩液晶显示屏，在全视角范围内皆可看到清晰的气道图像。 \n3.连接部位采用双环卡槽式设计，以避免图像传输中断。 \n4.显示器：能上下0°~130°转动，左右0°~270°转动，显示器尺寸≥3.0寸。\n5.内置全密封防水设计的高功率LED光源，能够清晰照亮口咽部的结构。\n6.防雾效果显著。                                                                     7.配套一次性使用喉片。",3,"台"]
[null,"可视喉镜（小儿）","\n1.显示器能：上下0°～130°转动，左右0°～270°转动\n2.喉镜片可插入镜片长度：幼儿≤70mm，儿童≤80mm\n3.镜片前端厚度：幼儿≤9.5mm，儿童≤10.5mm\n4.镜片角度：幼儿≤27度，儿童≤28度\n5.视场角：≤60°±15%\n6.摄像头内置的全密封防水设计高功率LED光源\n光照度：≥150Lux,≤500 Lux\n7.配套一次性使用喉片。\n",1,"台"]
["总计",null,null,{"$f":"SUM(D3:D6)","v":7}]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}