{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["报价表"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"报价表","index":0,"n_rows":71,"n_cols":8,"rows_kept":71,"merged":[[0,0,0,7],[1,0,1,7],[2,0,2,7],[36,1,36,7],[55,0,55,7],[62,0,62,7],[70,1,70,7]],"flags":["formulas_cached_only"]}
["报价表"]
["项目名称：郁南县第二人民医院神经康复病区建设项目（医用中心供氧、负压吸引、呼叫系统、医用扶手、医用床帘、输液杆等采购）"]
["一  中心供氧部分"]
["序号","产品名称","规格型号","单位","数量","单价","总价","备注"]
[1,"铝合金设备带","200*55*1.5mm","m",162]
[2,"脱脂紫铜管","支管8X1.0mm","m",230]
[3,"脱脂紫铜管","横支管22X1.0mm","m",102]
[4,"脱脂紫铜管","主管35x2.0mm","m",110]
[5,"汽化器","200立方","台",1]
[6,"调压阀组","200立方","套",1]
[7,"低温汇流排","4瓶组","套",1]
[8,"氧气终端","国标","套",84]
[9,"房间维修阀","004型","个",32]
[10,"双气报警器","灯光声音","套",2]
[11,"二级稳压箱","双路","套",3]
[12,"氧气流量计",null,"套",2]
[13,"楼层阀","DN20","个",3]
[14,"灯管","LED","套",84]
[15,"插座","五孔10A","个",168]
[16,"堵头","塑料","个",56]
[17,"电源线","2.5平方","m",600]
[18,"防尘盖","PVC","个",84]
[19,"灯罩","塑料L=30mm","个",84]
[20,"漏电开关","1p+N","个",28]
[21,"线槽","#39","m",80]
[22,"脱脂紫铜弯头","*35X1.5","个",12]
[23,"脱脂紫铜弯头","*22x1.5","个",18]
[24,"脱脂紫铜弯头","*15X1.0","个",18]
[25,"脱脂紫铜三通","*35X1.5","个",5]
[26,"脱脂紫铜三通","*22X1.5","个",22]
[27,"脱脂紫铜三通","*15X1.0","个",28]
[28,"脱脂紫铜三通","*8X1.0","个",87]
[29,"脱脂紫铜直接","*35X1.5","个",25]
[30,"脱脂紫铜直接","*22X1.5","个",23]
[31,"脱脂紫铜直接","*15X1.0","个",58]
[24,"小计"]
[null,"二  负压吸引部分"]
[1,"真空泵","水循环式4.5千瓦","台",2]
[2,"水箱","0.5立方","套",1]
[3,"储气罐","0.5立方","个",1]
[4,"电控柜","自动，手动","套",1]
[5,"脱脂紫铜管","主管/42*1.5mm","m",36]
[6,"脱脂紫铜管","横支管28X1.5mm","m",102]
[7,"脱脂紫铜管","负压支管/10*1.0mm","m",298]
[8,"负压终端","国标","个",84]
[1,"脱脂紫铜弯头","*42X1.5","个",12]
[2,"脱脂紫铜弯头","*28X1.5","个",26]
[3,"脱脂紫铜弯头","*10X1.0","个",87]
[4,"脱脂紫铜三通","*42X1.5","个",5]
[5,"脱脂紫铜三通","*28X1.5","个",32]
[6,"脱脂紫铜三通","*10X1.0","个",120]
[7,"脱脂紫铜直接","*42X1.5","个",18]
[8,"脱脂紫铜直接","*28X1.5","个",36]
[9,"脱脂紫铜直接","*10X1.0","个",84]
[null,"小计"]
["                         三   信息化呼叫系统部分"]
[1,"呼叫主机","JSY-5288K","台",2]
[2,"走廊显示屏","JSY-18","套",6]
[3,"床头分机","HX-858","台",84]
[4,"卫生间紧急分机","HX-808","个",28]
[5,"呼叫线","1.5平方","米",680]
[6,"小计"]
["     四   隔帘导轨、输液杆、走廊扶手（防撞带）部分"]
[1,"隔帘导轨+防火隔帘布","L2300X1800","套",84]
[2,"输液导轨","1.8米","条",84]
[3,"不锈钢输液吊杆","2米","条",84]
[4,"导轨固定支架","3+4木方","米",504]
[5,"走廊扶手","159型","米",264]
[6,"小计"]
[null,"总计"]
[null,"大写：元整。       小写￥0元整"]