{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["2-1新增材料单价确认表(信息价）安装工程 "],"not_rendered":{"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"2-1新增材料单价确认表(信息价）安装工程 ","index":0,"n_rows":72,"n_cols":6,"rows_kept":72,"merged":[[0,0,0,5]]}
["高低压配电工程及地下室-强电工程"]
["序号","材料/设备名称","规格、型号","计量\n单位","暂估工程量","备注"]
[1,"铜芯电缆 ","ZR-YJY-8.7/15kV-3x120mm2","m",159.883]
[2,"铜芯电缆"," WDUZN-YJY-1x185","m",44.7834]
[3,"电缆桥架  ","10kV电缆桥架    CT-300x150*1.5","m",37.191]
[4,"插接母线槽 五芯密集型铜芯封闭母线"," I-LINE-C-3150A 三相四线 3L+N+PE （5P）","m",{"$f":"95.03+12.77","v":107.8}]
[5,"母线槽始端箱"," I-LINE-C-3150A（5P）","台",{"$f":"7+1","v":8}]
[6,"母线槽终端箱 ","I-LINE-C-3150A（5P）","台",{"$f":"7+1","v":8}]
[7,"垂直弯头 ","3150A(5P,IP54)","个",{"$f":"14+2","v":16}]
[8,"母线槽支架 ","3150A(5P,IP54)","个",{"$f":"48+7","v":55}]
[9,"软连接 ","3150A(5P,IP54)","个",{"$f":"14+2","v":16}]
[10,"低压配电柜(屏) 消防负荷配电柜 1AN1","GCS，详见系统图","台",1]
[11,"低压配电柜(屏) 消防负荷配电柜 1AN2","GCS，详见系统图","台",1]
[12,"低压配电柜(屏) 消防负荷配电柜 1AN3","GCS，详见系统图","台",1]
[13,"低压配电柜(屏) 双电源转换联络柜（市电-发电机） 1AN4","GCS，详见系统图","台",1]
[14,"低压配电柜(屏) 联络配电柜 1AN5","GCS，详见系统图","台",1]
[15,"低压配电柜(屏) 电能质量综合治理一体柜 1AN6","GCS，详见系统图","台",1]
[16,"低压配电柜(屏) 电能质量综合治理一体柜 1AN7","GCS，详见系统图","台",1]
[17,"低压配电柜(屏) 一级及重要负荷配电柜 1AN8","GCS，详见系统图","台",1]
[18,"低压配电柜(屏) 一级及重要负荷配电柜 1AN9","GCS，详见系统图","台",1]
[19,"低压配电柜(屏) 一般负荷配电柜 1AN10","GCS，详见系统图","台",1]
[20,"低压配电柜(屏) 一级及重要负荷配电柜 1AN11","GCS，详见系统图","台",1]
[21,"低压配电柜(屏) 一级及重要负荷配电柜 1AN12","GCS，详见系统图","台",1]
[22,"低压配电柜(屏) 联络配电柜 1AN13","GCS，详见系统图","台",1]
[23,"低压配电柜(屏) 一般负荷配电柜 2AN1","GCS，详见系统图","台",1]
[24,"低压配电柜(屏) 一般负荷配电柜 2AN2","GCS，详见系统图","台",1]
[25,"低压配电柜(屏) 一般负荷配电柜 2AN3","GCS，详见系统图","台",1]
[26,"低压配电柜(屏) 一般负荷配电柜 2AN4","GCS，详见系统图","台",1]
[27,"低压配电柜(屏) 电能质量综合治理一体柜 2AN5","GCS，详见系统图","台",1]
[28,"低压配电柜(屏) 电能质量综合治理一体柜 2AN6","GCS，详见系统图","台",1]
[29,"低压配电柜(屏) 联络配电柜 2AN7","GCS，详见系统图","台",1]
[30,"低压配电柜(屏) 消防负荷配电柜 2AN8","GCS，详见系统图","台",1]
[31,"低压配电柜(屏) 消防负荷配电柜 2AN9","GCS，详见系统图","台",1]
[32,"低压配电柜(屏) 消防负荷配电柜 2AN10","GCS，详见系统图","台",1]
[33,"低压配电柜(屏) 双电源转换联络柜（市电-发电机） 2AN11","GCS，详见系统图","台",1]
[34,"低压配电柜(屏) 一级及重要负荷配电柜 2AN12","GCS，详见系统图","台",1]
[35,"低压配电柜(屏) 一级及重要负荷配电柜 2AN13","GCS，详见系统图","台",1]
[36,"低压配电柜(屏) 联络配电柜 3AN1","GCS，详见系统图","台",1]
[37,"低压配电柜(屏) 电能质量综合治理一体柜 3AN2","GCS，详见系统图","台",1]
[38,"低压配电柜(屏) 电能质量综合治理一体柜 3AN3","GCS，详见系统图","台",1]
[39,"低压配电柜(屏) 一级及重要负荷配电柜 3AN4","GCS，详见系统图","台",1]
[40,"低压配电柜(屏) 一级及重要负荷配电柜 3AN5","GCS，详见系统图","台",1]
[41,"低压配电柜(屏) 一级及重要负荷配电柜 3AN6","GCS，详见系统图","台",1]
[42,"低压配电柜(屏) 一级及重要负荷配电柜 3AN7","GCS，详见系统图","台",1]
[43,"低压配电柜(屏) 一级及重要负荷配电柜 3AN8","GCS，详见系统图","台",1]
[44,"低压配电柜(屏) 联络配电柜 3AN9","GCS，详见系统图","台",1]
[45,"低压配电柜(屏) 一级及重要负荷配电柜 4AN1","GCS，详见系统图","台",1]
[46,"低压配电柜(屏) 一级及重要负荷配电柜 4AN2","GCS，详见系统图","台",1]
[47,"低压配电柜(屏) 双电源转换联络柜（市电-发电机） 4AN3","GCS，详见系统图","台",1]
[48,"低压配电柜(屏) 一般负荷配电柜 4AN4","GCS，详见系统图","台",1]
[49,"低压配电柜(屏) 一般负荷配电柜 4AN5","GCS，详见系统图","台",1]
[50,"低压配电柜(屏) 一般负荷配电柜 4AN6","GCS，详见系统图","台",1]
[51,"低压配电柜(屏) 一般负荷配电柜 4AN7","GCS，详见系统图","台",1]
[52,"低压配电柜(屏) 电能质量综合治理一体柜 4AN8","GCS，详见系统图","台",1]
[53,"低压配电柜(屏) 电能质量综合治理一体柜 4AN9","GCS，详见系统图","台",1]
[54,"低压配电柜(屏) 联络配电柜 4AN10","GCS，详见系统图","台",1]
[55,"低压开关柜(屏) ","GCS，详见系统图","台",1]
[56,"直流屏 ZLP 65Ah/110V","详见系统图","台",1]
[57,"高压配电柜 高压进行柜 AK1","KYN28-12，详见系统图","台",1]
[58,"高压配电柜 高压计量柜 AK2","KYN28-12，详见系统图","台",1]
[59,"高压配电柜 高压出线柜 AK3","KYN28-12，详见系统图","台",1]
[60,"高压配电柜 高压出线柜 AK4","KYN28-12，详见系统图","台",1]
[61,"高压配电柜 高压联络柜 AK5","KYN28-12，详见系统图","台",1]
[62,"高压配电柜 高压隔离提升柜 AK6","KYN28-12，详见系统图","台",1]
[63,"高压配电柜 高压出线柜 AK7","KYN28-12，详见系统图","台",1]
[64,"高压配电柜 高压出线柜 AK8","KYN28-12，详见系统图","台",1]
[65,"高压配电柜 高压计量柜 AK9","KYN28-12，详见系统图","台",1]
[66,"高压配电柜 高压进线柜 AK10","KYN28-12，详见系统图","台",1]
[67,"低压配电柜(屏) 低压进线柜 FAN1","GGD，，详见系统图","台",1]
[68,"低压配电柜(屏) 一级及重要负荷配电柜 FAN2","GGD，，详见系统图","台",1]
[69,"低压配电柜(屏) 消防负荷配电柜 FAN3","GGD，，详见系统图","台",1]
[70,"干式变压器 ","SCB13（H)-NX2-1600kVA Dyn11,Ud=6% R＜1欧 配帘式风扇 带IP30防护外壳","台",4]