{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["人防工程设备设施"],"not_rendered":{"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"人防工程设备设施","index":0,"n_rows":32,"n_cols":6,"rows_kept":32,"merged":[[0,0,0,5]]}
["人防工程设备设施清单"]
["序号","材料/设备名称","规格、型号","计量\n单位","暂估工程量","报价（元）"]
[1,"钢结构活门槛双扇防护密闭门GHSFM5025(5)","1.钢结构活门槛双扇防护密闭门-防护等级5\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":2,"d":"2.00"}]
[2,"钢结构活门槛双扇防护密闭门GHSFM5025(6)","1.钢结构活门槛双扇防护密闭门-防护等级6\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":1,"d":"1.00"}]
[3,"钢结构双扇防护密闭门GSFM5528(5)","1.钢结构双扇防护密闭门-防护等级5\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":1,"d":"1.00"}]
[4,"连通口双向受力双扇防护密闭门GSFMG5025(5)","1.钢结构双扇防护双向受力密闭门-防护等级5\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":1,"d":"1.00"}]
[5,"连通口双向受力双扇防护密闭门GSFMG6025(5)","1.钢结构双扇防护双向受力密闭门-防护等级5\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":3,"d":"3.00"}]
[6,"连通口双向受力双扇防护密闭门GSFMG6025(6","1.钢结构双扇防护双向受力密闭门-防护等级6\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":1,"d":"1.00"}]
[7,"钢筋混凝土单扇防护密闭门HFM0820(5)","1.钢筋混凝土单扇防护密闭门-防护等级5\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":7,"d":"7.00"}]
[8,"钢筋混凝土单扇防护密闭门HFM0820(6)","1.钢筋混凝土单扇防护密闭门-防护等级6\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":6,"d":"6.00"}]
[9,"钢筋混凝土单扇防护密闭门HFM1220(5)","1.钢筋混凝土单扇防护密闭门-防护等级5\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":1,"d":"1.00"}]
[10,"钢筋混凝土单扇防护密闭门HFM1220(6)","1.钢筋混凝土单扇防护密闭门-防护等级6\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":5,"d":"5.00"}]
[11,"钢筋混凝土单扇防护密闭门HFM1520(5)","1.钢筋混凝土单扇防护密闭门-防护等级5\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":3,"d":"3.00"}]
[12,"钢筋混凝土活门槛单扇防护密闭门HHFM1220(5)","1.钢筋混凝土活门槛单扇防护密闭门-防护等级5\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":2,"d":"2.00"}]
[13,"钢筋混凝土活门槛单扇防护密闭门HHFM1220(6)","1.钢筋混凝土活门槛单扇防护密闭门-防护等级6\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":1,"d":"1.00"}]
[14,"钢筋混凝土活门槛单扇防护密闭门HHFM1520(5)","1.钢筋混凝土活门槛单扇防护密闭门-防护等级5\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":1,"d":"1.00"}]
[15,"钢筋混凝土活门槛单扇防护密闭门HHFM1520(6)","1.钢筋混凝土活门槛单扇防护密闭门-防护等级6\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":3,"d":"3.00"}]
[16,"钢筋混凝土活门槛单扇密闭门HHM1220","1.钢筋混凝土活门槛单扇密闭门\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":2,"d":"2.00"}]
[17,"钢筋混凝土活门槛单扇密闭门HHM1520","1.钢筋混凝土活门槛单扇密闭门\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":4,"d":"4.00"}]
[18,"钢筋混凝土单扇密闭门HM0716","1.钢筋混凝土单扇密闭门0716\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":4,"d":"4.00"}]
[19,"钢筋混凝土单扇密闭门HM0820","1.钢筋混凝土单扇密闭门0820\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":7,"d":"7.00"}]
[20,"钢筋混凝土单扇密闭门HM1020","1.钢筋混凝土单扇密闭门1020\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":3,"d":"3.00"}]
[21,"钢筋混凝土单扇密闭门HM1220","1.钢筋混凝土单扇密闭门1220\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":7,"d":"7.00"}]
[22,"钢筋混凝土单扇密闭门HM1520","1.钢筋混凝土单扇密闭门\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":3,"d":"3.00"}]
[23,"防爆波活门BMH11000-30","1.防爆波活门-通风量11000m3/h-门扇压力值0.3MPa\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":2,"d":"2.00"}]
[24,"防爆波活门BMH14500-30","1.防爆波活门-通风量14500m3/h-门扇压力值0.3MPa\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":18,"d":"18.00"}]
[25,"防爆波活门BMH5700-30","1.防爆波活门-通风量5700m3/h-门扇压力值0.3MPa\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":1,"d":"1.00"}]
[26,"防爆波活门BMH8000-15","1.防爆波活门-通风量8000m3/h-门扇压力值0.15MPa\n2.在洞内、地下室内、库内或暗室内进行施工","樘",{"v":4,"d":"4.00"}]
[27,"密闭观察窗MGC1008",null,"樘",{"v":1,"d":"1.00"}]
[28,"维修吊环Φ20",null,"个",{"v":76,"d":"76.00"}]
[29,"维修吊环Φ25",null,"个",{"v":36,"d":"36.00"}]
[30,"人防标识牌",null,"套",{"v":4,"d":"4.00"}]